[Contents] [Prev] [Next] [Index] [Report an Error]

# show qos scheduler-hierarchy

#### Syntax

To display information about the scheduler hierarchy on a specified interface:

show qos scheduler-hierarchy interfaceType interfaceSpecifier
[ atmVpi | s-vlanIdValue ] [ explicit | level levelNumber ]
[ traffic-class-group { trafficClassGroupName | default } ] [ brief | full | summary ]
[ filter ]

To display information about the scheduler hierarchy on a specified tunnel-service interface:

show qos scheduler-hierarchy tunnel-server interfaceType [ explicit |
level levelNumber ] [ traffic-class-group { trafficClassGroupName | default } ] [ brief | full | summary ] [ filter ]

To display information about the scheduler hierarchy on a specified L2TP session:

show qos scheduler-hierarchy lt2p session sessionName [ explicit | level levelNumber ] [ traffic-class-group { trafficClassGroupName | default } ] [ brief | full | summary ] [ filter ]

To display information about the scheduler hierarchy for an interface set:

show qos scheduler-hierarchy qos-interface-set interfaceSetName [ full | brief | summary ] [ filter ]

To display information about the scheduler hierarchy for an interface superset:

show qos scheduler-hierarchy qos-interface-superset interfaceSupersetName [ full | brief | summary ] [ filter ]

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

qos-interface-set keyword and interfaceSetName variable added in JUNOSe Release 9.2.0.

qos-interface-superset keyword and interfaceSupersetName variable added in JUNOSe Release 9.2.0.

#### Description

Displays information about the scheduler hierarchy on a specified interface, L2TP session, or tunnel-service interface.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- atmVpi—Virtual path identifier of this PVC; number in the range 0–255
- s-vlanIdValue—S-VLAN ID number in the range 0–4095
- explicit—Displays scheduler profiles for the specified interface rather than those stacked above the interface
- levelNumber—Number of scheduler levels above specified interface to report; 0 indicates the specified interface
- trafficClassGroupName—Name of the traffic-class group for which to display the scheduler hierarchy
- sessionName —Name of the L2TP session
- interfaceSetName—Name of the interface set
- interfaceSupersetName—Name of the interface superset
- default—Displays the scheduler hierarchy of the default traffic-class group
- brief—Displays information in condensed format
- full—Displays information in expanded format
- summary—Displays summary of scheduler profiles stacked above the specified interface
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Monitoring the QoS Scheduler Hierarchy

[Contents] [Prev] [Next] [Index] [Report an Error]