[Contents] [Prev] [Next] [Index] [Report an Error]

# full-spf-always

#### Syntax

[ no ] full-spf-always

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables full SPF calculations for ISIS network changes. The no version restores partial route calculation (PRC) mode for SPF calculations.

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]