[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Queue Statistics for the Fabric

#### Purpose

Display forwarded and dropped statistics for the fabric.

#### Action

To display general information about the fabric queue:

    host1#show fabric-queue
      traffic     egress               forwarded   forwarded   dropped   dropped
       class       slot      type       packets      bytes     packets    bytes
    -----------   ------   ---------   ---------   ---------   -------   -------
    best-effort    all     committed       0           0          0         0
    best-effort    all     conformed       0           0          0         0
    best-effort    all     exceeded        0           0          0         0

To display detailed information about the fabric queue in a specific traffic class:

    host1#show fabric-queue traffic-class video detail

To display information about the fabric queue on the egress slot:

    host1#show fabric-queue egress-slot 0

#### Meaning

Table 45 lists the show fabric-queue command output fields.

Table 45: show fabric-queue Output Fields

Field Name | Field Description
--- | ---
traffic class | Name of the traffic class
egress slot | Egress slot for which statistics are being displayed
type | Type of packet
forwarded packets | Number of forwarded packet
forwarded bytes | Number of forwarded bytes
dropped packets | Number of dropped packets
dropped bytes | Number of dropped bytes

#### Related Topics

- Configuring Rate Statistics
- Configuring Event Statistics
- show fabric-queue command

[Contents] [Prev] [Next] [Index] [Report an Error]