[Contents] [Prev] [Next] [Index] [Report an Error]

# ip multipath round-robin

#### Syntax

[ no ] ip multipath round-robin

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies round-robin as the mode for ECMP load sharing on an interface. The no version restores the default value, hashed.

#### Mode

Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]