[Contents] [Prev] [Next] [Index] [Report an Error]

# baseline ip igmp

#### Syntax

baseline ip igmp

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets a baseline for IGMP statistics. The router implements the baseline by reading and storing the statistics at the time the baseline is set and then subtracting this baseline whenever baseline-relative statistics are retrieved. There is no no version.

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]