[Contents] [Prev] [Next] [Index] [Report an Error]

# ip vrrp preempt

#### Syntax

[ no ] ip vrrp vrid preempt

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables VRRP preemption. The no version disables VRRP preemption. The default is enabled.

#### Options

- vrid—VRID identifier; a number in the range 1–255

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]