[Contents] [Prev] [Next] [Index] [Report an Error]

# aaa authorization

#### Syntax

aaa authorization { exec | commands level } authorListName authMethod
[ authMethod ]*

no aaa authorization { exec | commands level } authorListName

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets parameters that restrict a user's access to a network. The no version disables authorization for a function.

#### Options

- exec—Runs authorization to determine if the user is allowed to run Exec mode commands
- level—Privilege level of commands for which authorization is run; in the range 0–15
- authorListName—Name of the authorization methods list of up to 32 characters
- authMethod—Authorization method:
  - if-authenticated—Allows the user to access the requested function if the user is authenticated
  - none—NAS does not request authorization information; authorization is not performed over this line
  - tacacs+—NAS exchanges authorization information with the TACACS+ security daemon
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]