[Contents] [Prev] [Next] [Index] [Report an Error]

# snmp-server notificationLog entryLimit

#### Syntax

snmp-server notificationLog entryLimit entryLimit

no snmp-server notificationLog entryLimit

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the maximum number of notifications kept. The no version returns the limit to the default value, 500.

#### Options

- entryLimit—Maximum number of notifications kept, in the range 1–500; default value is 500

  | Note: You can allocate up to 500 notifications across all virtual routers on the router. As you allocate entry limits for virtual routers, the available range changes to reflect the number of notifications that you have allocated.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]