[Contents] [Prev] [Next] [Index] [Report an Error]

# ip directed-broadcast

#### Syntax

[ no ] ip directed-broadcast

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables translation of directed broadcast to physical broadcasts. The no version disables the function.

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]