[Contents] [Prev] [Next] [Index] [Report an Error]

# atm sonet stm-1

#### Syntax

[ no ] atm sonet stm-1

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the mode of operation on the physical interface to SDH STM-1. The no version restores the default value, SONET STS-3c operation.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]