[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 mld access-group

#### Syntax

ipv6 mld access-group accessListName

no ipv6 mld access-group

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Restricts hosts on this subnet to joining multicast groups on the specified IPv6 access list. The no version removes the association with the specified access list and allows hosts on the subnetwork to join any multicast group.

#### Options

- accessListName—Name of the access list; a string of up to 32 characters

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]