> - Download PDFs
> - sscc transportRouter

> # sscc transportRouter

> #### Syntax

> sscc transportRouter name

> no sscc transportRouter [ name ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Configures the router on which the TCP/COPS connection is to be established. The no version removes the SRC client transport router.

> #### Options

> - name—Name of a transport router

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.