[Contents] [Prev] [Next] [Index] [Report an Error]

# l2c ip oif

#### Syntax

[ no ] l2c ip oif

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Creates an IGMP session at the virtual router within the context. ANCP needs IGMP sessions so it can convey OIF mapping events to the appropriate ANCP neighbor. The no version removes the IGMP session.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]