> - Download PDFs
> - radius nas-port-format

> # radius nas-port-format

> #### Syntax

> radius nas-port-format { 0ssssppp | ssss0ppp }

> no radius nas-port-format

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Configures the RADIUS client’s use of a specific format for RADIUS attribute 5, NAS-Port. The no version removes the format.

> #### Options

> - 0ssssppp—Sets the RADIUS client to use the 0ssssppp format where s is slot and p is port
> - ssss0ppp—Sets the RADIUS client to use the ssss0ppp format where s is slot and p is port

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.