[Contents] [Prev] [Next] [Index] [Report an Error]

# Clearing and Re-Creating Dynamic Interfaces from MPLS Major Interfaces

To remove and re-create dynamic IPv4 interfaces and dynamic IPv6 interfaces from all MPLS major interfaces or a specific MPLS major interface:

- Issue the clear mpls dynamic-interfaces on-major-interfaces command:
  `
  host1#clear mpls dynamic-interfaces on-major-interfaces
  `

You can use this command to reapply policies related to dynamic IPv4 and IPv6 interfaces on top of MPLS major interfaces.

There is no no version.

#### Related Topics

- clear mpls dynamic-interfaces on-major-interfaces

[Contents] [Prev] [Next] [Index] [Report an Error]