> - Download PDFs
> - show l2tp dial-out target

> # show l2tp dial-out target

> #### Syntax

> show l2tp dial-out target [ targetIpAddress targetIpAddressMask | allVirtualRouters ]
> [ detail ] [ state operState ] [ filter ]

> To display summary information:

> show l2tp dial-out target summary [ allVirtualRouters ] [ filter ]

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Displays configured dial-out targets within the current virtual router context.

> #### Options

> - targetIpAddress—Trigger IP address for the target that you want to display
> - targetIpAddressMask—Mask for the trigger IP address
> - allVirtualRouters—Displays dial-out information for all virtual routers
> - detail—Displays configuration, state, and statistics
> - operState—One of the following operational states:
>   - down
>   - inService
>   - inhibited
> - filter—See Filtering show Commands
> - summary—Displays aggregate counts for targets in each of the possible operational and administrative states

> #### Mode

> Privileged Exec

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.