[Contents] [Prev] [Next] [Index] [Report an Error]

# ip multicast-routing disable-rpf-check

#### Syntax

ip multicast-routing disable-rpf-check ipAccessList

no ip multicast-routing disable-rpf-check

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Disables RPF checks for the (S,G) pairs in the specified access list. The no version restores the default situation, in which the router performs RPF checks for all (S,G) pairs.

#### Options

- ipAccessList—Name of the IP access list that specifies the (S,G) pairs

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]