[Contents] [Prev] [Next] [Index] [Report an Error]

# threshold-test

#### Syntax

threshold-test startup { falling | rising | risingorfalling }

threshold-test absolute-value rising risingValue falling fallingValue

threshold-test event { rising eventOwner eventName | falling eventOwner eventName | delta-rising eventOwner eventName | delta-falling eventOwner eventName }

threshold-test delta-value rising risingValue falling fallingValue

no threshold-test [ startup | absolute-value | delta-value | event rising | event falling | event delta-rising | event delta-falling ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Defines the values for an SNMP threshold-test trigger. The no version deletes the threshold-test values for this trigger or removes either the threshold startup condition or event binding.

#### Options

- startup—Startup threshold condition that you predict the sample to follow
  - falling—Specifies that the sample values are expected to be falling values
  - rising—Specifies that the sample values are expected to be rising values
  - risingorfalling—Specifies that the sample values might be either rising values or falling values
- absolute-value—Specifies that the trigger is monitoring absolute threshold values
- risingValue—Rising threshold value for the trigger, in the range -2147483648–2147483648
- fallingValue—Falling threshold value for the trigger, in the range -2147483648–2147483648
- event—Binds an event owner and name to specific events on which the threshold-test might trigger: rising values within a sample, falling values within a sample, rising values between samples, or falling values between samples
- eventOwner—Event owner name; string of up to 32 alphanumeric characters
- eventName—Event name; string of up to 32 alphanumeric characters
- delta-value—Specifies that the trigger is monitoring the difference (delta)( between sample values

#### Mode

SNMP Trigger Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]