[Contents] [Prev] [Next] [Index] [Report an Error]

# l2tp shutdown destination

#### Syntax

[ no ] l2tp shutdown destination { destinationName |
[ virtual-router vrName ] ip ipAddress }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Closes all tunnels and sessions at a destination, and prevents the creation of new tunnels and sessions at that destination. This command works in conjunction with the l2tp drain destination command. Both commands affect the status of the administrative state of L2TP on the destination; the l2tp shutdown destination command sets the administrative state to disabled. The no version enables the creation of new tunnels and sessions at that destination.

#### Options

- destinationName—Name the router assigns to the LNS
- vrName—Name of the virtual router on which the destination exists
- ipAddress—IP address of the LNS

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]