[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Interfaces That are Synchronizing with LDP

Purpose

Display information about interfaces that are synchronizing with LDP or the specified interface that is synchronizing with LDP.

Action

To display information about interfaces synchornizing with LDP:

    host1#show ldp igp-sync
    Atm 0/0:
           LDP configured;  SYNC enabled.
           SYNC status: sync achieved; peer reachable.
           IGP holddown time: infinite.
           Peer LDP Ident: 10.130.0.1:0
           IGP enabled: OSPF 1

Meaning

Table 36 lists the show ldp igp-sync command output fields.

Table 36: show ldp igp-sync Output Fields

Field Name | Field Description
--- | ---
LDP | State of LDP, configured, auto-configured, or not configured
SYNC status | State of synchronization, enabled or disabled
IGP holddown time | Value of IGP hold down time, infinite or number of milliseconds
Peer LDP Ident | IP address of LDP peer
IGP enabled | IGP protocol

#### Related Topics

- show ldp igp-sync

[Contents] [Prev] [Next] [Index] [Report an Error]