[Contents] [Prev] [Next] [Index] [Report an Error]

# ip local pool warning

#### Syntax

ip local pool name warning highUtilization abatedUtilization [ snmpTrap ]

no ip local pool name warning [ highUtilization abatedUtilization ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Identifies the warning threshold values. The no version resets the thresholds to their default values.

#### Options

- name—Text string in the range 1–16 characters that defines the name of the local address pool
- highUtilization—High utilization value; a number in the range 1–100; default value is 85
- abatedUtilization—Abated utilization value; a number in the range 1–100; default value is 75
- snmpTrap—Enables snmp pool utilization traps

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]