[Contents] [Prev] [Next] [Index] [Report an Error]

# ip dhcp-external disregard-giaddr-next-hop

#### Syntax

[ no ] ip dhcp-external disregard-giaddr-next-hop

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the DHCP external application to disregard the giaddr in packets destined for the DHCP server when the next hop for a subscriber's access route is determined. The no version returns to the default, in which DHCP external uses the giaddr to determine the next hop.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]