[Contents] [Prev] [Next] [Index] [Report an Error]

# link selection

#### Syntax

link selection { primary | secondary }

no link selection

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Disables redundancy on a GE I/O module by allowing operation on the specified port only. The no version restores the default situation, in which port redundancy is enabled.

#### Options

- primary—Allows operation on only the primary port
- secondary—Allows operation on only the redundant port

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]