[Contents] [Prev] [Next] [Index] [Report an Error]

# clear bgp ipv6 wait-end-of-rib

#### Syntax

clear bgp ipv6 [ unicast | multicast | vpnv6 | route-target signaling ] [ vrf vrfName ]
[ ipAddress | ipv6Address | peer-group peerGroupName | * ] wait-end-of-rib

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
ipv6Address variable added in JUNOSe Release 8.0.0.
route-target signaling keywords added in JUNOSe Release 8.2.0.

#### Description

Resets the IPv6 BGP session and brings down the underlying TCP connection and then brings it back up again, causing both peers to resend their complete BGP routing table. Clears the specified peer from the set of peers for which BGP is waiting to receive an End-of-RIB marker after a peer restart. Hard clearing a peer has the same effect for that peer. There is no no version.

#### Options

- unicast—Clears the unicast routing table; the default option
- multicast—Clears the multicast routing table
- vpnv6 —Clears the VPNv6 unicast routing and forwarding table
- route-target signaling—Clears the route-target membership information
- vrfName—Name of a virtual routing and forwarding instance to clear
- ipAddress—IP address of identified BGP neighbor to clear
- ipv6Address—IPv6 address of identified BGP neighbor to clear
- peerGroupName—Name of a BGP peer group to clear
- *—Clears all connections

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]