[Contents] [Prev] [Next] [Index] [Report an Error]

# bulkstats schema subtree

#### Syntax

bulkstats schema schemaIndex subtree
{ if-stack | if-stats { subtreelist [ ifstatsList [ ifstatsList ]* ] |
if-create-delete-time-stats interfaceType interfaceType } | igmp | system }

bulkstats schema schemaIndex subtree
{ if-stack | if-stats | igmp [ subtreelist igmpList [ igmpList ]* ] | system }

no bulkstats schema schemaIndex

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
mplsL2shim, mplsMajor, and mplsMinor keywords added in JUNOSe Release 8.2.0.

#### Description

Configures the schema for collecting if-stack, if-stats, or router data. The no version removes the schema.

#### Options

- schemaIndex—Identifier for the schema in the range 1–65535
- if-stack—Retrieves ifStackTable
- if-stats—Retrieves ifTable/ifXTable counters
- ifstatsList—Type of statistics and time-offset keyword, which includes the offset from the master interval at which the record was collected in each bulkstats interface record
- if-create-delete-time-stats—Retrieves interface final statistics (interface statistics that may be lost during higher create or delete frequency)
- interfaceType—One of the following interface types for which you can collect statistics: ATM 1483, IP, MPLS minor, MPLS major, MPLS shim, PPP
- igmp—Retrieves IGMP statistics
- igmpList—Type of statistics and time-offset keyword, which includes the offset from the master interval at which the record was collected in each bulkstats interface record
- system—Retrieves sysUpTime and nvsUtilPct global statistics; retrieves slotDescr, the cpuUtilPct, and memUtilPct per-slot statistics
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]