[Contents] [Prev] [Next] [Index] [Report an Error]

# Clearing Dynamic MAC Addresses from the VPLS Forwarding Table

You can use the following clear commands to remove all dynamic (learned) MAC address entries or a specific dynamic MAC address entry from the forwarding table for a VPLS instance.

Tasks to clear the VPLS forwarding table are:

- Clearing All Dynamic MAC Addresses from the VPLS Forwarding Table
- Clearing a Specific Dynamic MAC Address from the VPLS Forwarding Table
- Clearing All Dynamic MAC Addresses for a Network Interface Associated with a VPLS Instance from the VPLS Forwarding Table
- Clearing All Dynamic MAC Addresses for the VPLS Virtual Core Interface Associated with A VPLS Instance

## Clearing All Dynamic MAC Addresses from the VPLS Forwarding Table

To clear all dynamic MAC address entries for the VPLS instance:

- Issue the clear bridge command.
  `
  host1#clear bridge vplsB
  `

There is no no version.

## Clearing a Specific Dynamic MAC Address from the VPLS Forwarding Table

To clear a specific dynamic MAC address entry for the VPLS instance:

- Issue the clear bridge address command.
  `
  host1#clear bridge vplsB address 0090.1a40.9992
  `

There is no no version.

## Clearing All Dynamic MAC Addresses for a Network Interface Associated with a VPLS Instance from the VPLS Forwarding Table

To clear all dynamic MAC address entries for a network interface associated with a VPLS instance:

- Issue the clear bridge interface command.
  `
  host1#clear bridge interface atm 3/3.2
  `

There is no no version.

## Clearing All Dynamic MAC Addresses for the VPLS Virtual Core Interface Associated with A VPLS Instance

To clear all dynamic MAC address entries for the VPLS virtual core interface associated with a VPLS instance:

- Issue the clear bridge interface vpls command.
  `
  host1#clear bridge interface vpls vplsA
  `

There is no no version.

#### Related Topics

- clear bridge
- clear bridge address
- clear bridge interface
- clear bridge interface vpls

[Contents] [Prev] [Next] [Index] [Report an Error]