[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls ldp graceful-restart reconnect-time

#### Syntax

mpls ldp graceful-restart reconnect-time [ seconds ]

no mpls ldp graceful-restart reconnect-time

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Specifies the length of time you want neighbors to wait for the gracefully restarting router to resume sending LDP messages to neighbors after the restart. The no version restores the default value, 120 seconds.

#### Options

- seconds—Number of seconds in the range 60–300

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]