[Contents] [Prev] [Next] [Index] [Report an Error]

# ipsec transport profile

#### Syntax

[ no ] ipsec transport profile { profileName [ [ virtual-router vrName ]
ip address ipAddress ] | [ virtual-router vrName ] ip address ipAddress }

no ipsec transport profile { profileName
| [ virtual-router vrName ] ip address ipAddress }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Creates or configures a transport profile for IPSec and accesses the IPSec Transport Profile Configuration mode. The no version deletes the transport profile.

#### Options

- profileName—Name of the transport profile
- vrName—Name of the VR on which you want to create the profile. If you do not specify a virtual router, the current virtual router context is used
- ipAddress—Remote endpoint for the IPSec transport connection. You can enter a single IP address or the wildcard address of 0.0.0.0. If you use the wildcard address, the profile accepts any remote client connection, which is a typical scenario for secure remote access.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]