[Contents] [Prev] [Next] [Index] [Report an Error]

# priority rate

#### Syntax

priority priorityValue rate rateValue

no priority priorityValue rate

#### Release Information

Command introduced in JUNOSe Release 8.1.0.

#### Description

Sets the rate for each priority. The no version returns to the default value.

#### Options

- priorityValue—Hi-Green-IC, Hi-Green-SC, Hi-Yellow-IC, Hi-Yellow-SC, Lo-Green-IC, Lo-Green-SC, Lo-Yellow-IC, Lo-Yellow-SC
- rateValue—Packets per second, in the range 64–65535

#### Mode

DoS Protection Group Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]