[Contents] [Prev] [Next] [Index] [Report an Error]

# color

#### Syntax

[ no ] [ suspend ] color { green | yellow | red }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Defines a policy rule that assigns a color to packets defined in the current classifier control list. The no version removes the rule from the policy list; the suspend version temporarily suspends the policy rule; the no suspend version resumes application of a suspended rule.

| Note: This command replaces the Policy List Configuration mode version of the color command, which may be removed completely in a future release.

#### Options

- green—Assigns green color to packets; highest precedence
- yellow—Assigns yellow color to packets; intermediate precedence
- red—Assigns red color to packets; lowest precedence

#### Mode

Classifier Group Configuration

#### Related Topics

- Hierarchical Rate Limits Overview
- Policy Rule Precedence

[Contents] [Prev] [Next] [Index] [Report an Error]