[Contents] [Prev] [Next] [Index] [Report an Error]

# domain-name

#### Syntax

From DHCP Local Pool Configuration mode:

domain-name domainName

no domain-name

From IPSec Identity Configuration mode:

[ no ] domain-name domainName

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

From DHCP Local Pool Configuration mode, specifies a domain name that can be returned to the subscriber of an address pool if requested. The no version removes the association between the address pool and the domain name.

From IPSec Identity mode, specifies the domain name that the router uses in IKE authentication messages and to generate certificate requests. The no version removes the domain name.

#### Options

- domainName—Name of the domain
- domainName—Name used in certificate requests and in IKE authentication messages; up to 60 characters

#### Mode

DHCP Local Pool Configuration, IPSec Identity Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]