[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 pim join-filter

#### Syntax

ipv6 pim join-filter accessListName

no ipv6 pim join-filter

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies an extended access list that you want this PIM router or PIM interface to use as a join filter. If an interface-level filter exists, it takes precedence over the global-level filter. The no version removes the filter association.

#### Options

- accessListName—Name of the access list that you want this interface to use as a PIM join filter; a string of up to 32 alphanumeric characters

#### Mode

Global Configuration, Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]