[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring IPv6 Local Pools for DHCP Prefix Delegation By All Configured Pools

#### Purpose

Display a summary of all the IPv6 local address pools configured on a virtual router, along with the prefix ranges in each of those pools, total number of prefixes that can be allocated to clients, and the number of prefixes that are in use by clients.

#### Action

To display information about all the IPv6 local address pools configured on a virtual router:

    host1#show ipv6 local pool
                                      IPv6 Local Address Pools
                                      ------------------------
          Pool                   Start                        End               Total    In Use
    ----------------   -------------------------   -------------------------   -------   -------
    ipv6Pool-pppoa     2002:2002::/48              2002:2002:ffff::/48         65536     0
    ipv6Pool-pppoe     3003:3003::/48              3003:3003:ffff::/48         65536     0
    example            4004:4004::/48              4004:4004:ffff::/48         65536     16000

#### Meaning

Table 33 lists the show ipv6 local pool command output fields.

Table 33: show ipv6 local pool Output Fields

Field Name | Field Description
--- | ---
Pool | Names of IPv6 local address pools configured on the virtual router
Start | Starting prefix of the range of prefixes configured in a particular pool
End | Ending prefix of the range of prefixes configured in a particular pool
Total | Number of prefixes available for allocation to clients from a particular pool
In Use | Number of prefixes in a pool that are currently used by DHCPv6 clients

#### Related Topics

- show ipv6 local pool

[Contents] [Prev] [Next] [Index] [Report an Error]