[Contents] [Prev] [Next] [Index] [Report an Error]

# ipv6 multicast-routing disable-rpf-check

#### Syntax

ipv6 multicast-routing disable-rpf-check accessListName

no ipv6 multicast-routing disable-rpf-check

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Disables RPF checks for the (S,G) pairs in the specified access list. The no version restores the default situation, in which the router performs RPF checks for all (S,G) pairs.

#### Options

- accessListName—Name of the IPv6 access list that specifies the (S,G) pairs

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]