[Contents] [Prev] [Next] [Index] [Report an Error]

# Using the CLI to Manage Subscriber Service Sessions

The CLI-based Service Manager creates static subscriber sessions and service sessions. You can also use CLI commands to immediately deactivate subscriber service sessions. The CLI-based support is particularly useful for:

- Testing your service definitions—for example, you might use the CLI commands to verify that a newly created service definition is correct. When you are satisfied with the service definition, you can then use RADIUS to activate the service for your subscribers.
- Preprovisioning Service Manager services—preprovisioning improves performance and efficiency by freeing Service Manager from having to repeatedly create and remove a service that you activate and deactivate for multiple subscribers. See Preprovisioning Services for more information about service preprovisioning.

## Using the CLI to Activate Subscriber Service Sessions

A subscriber session represents a specific subscriber—the session consists of the subscriber’s name, the interface used for the session, and any active services for the subscriber. A subscriber can have one subscriber session active at any given time.

You create a subscriber’s service session when you assign a service definition to a subscriber session. Like an AAA-created service, a single subscriber session can have multiple simultaneous service sessions. You can use one method to create the subscriber session, and then a different method to activate the subscriber’s service session. For example, you might use RADIUS to create the AAA subscriber session, then use the CLI to activate the service session for the subscriber, You can optionally specify a service session profile that you want to attach to the service session.

You can use the CLI to activate a service session based on subscriber information or owner information:

- Subscriber name and interface method—Activates the service session based on the subscriber name and the interface that the subscriber is using for this subscriber session.
  `
  host1(config)#service-management subscriber-session client1@isp1.com interface atm 4/0.1 service-session “ tiered(1280000, 5120000)”
  `
- Owner name and ID method—Activates the service session based on the owner that created the subscriber session and the ID that was generated by the owner. For example, if RADIUS is used to create the subscriber session, the owner name is AAA and the owner ID is the Acct-Session-ID that was generated by RADIUS during subscriber creation.
  `
  host1(config)#service-management owner-session AAA 537446 service-session “ tiered(1280000, 5120000)”
  `

  | Note: You must specify the parameter values in the order in which the parameters appear in the template name of the service definition file. Enclose the service definition name in double quotation marks, with the service’s parameter values in parentheses. For example, for the tiered service that is defined in Figure 27, the template name is: `<# tiered(inputBW, outputBW) #>` Use the following format with the service-session keyword: `“ tiered(1280000, 5120000)”`

service-management owner-session

- Use to activate a service for an existing subscriber by identifying the owner used to create the subscriber session and specifying the service session to use.
- The subscriber session must exist before you use this command.
- Use this command in Privileged Exec mode to create a dynamic subscriber session—dynamic sessions are deleted after a router reboot.
- Use this command in Global Configuration mode to create persistent subscriber sessions that are retained across reboots.
- Specify the name of the owner (the method originally used to create the subscriber session), and the ID generated by the of the owner. For example, if RADIUS was used to create the subscriber session, the owner name is AAA and the owner ID is the Acct-Session-ID generated by RADIUS when the subscriber session was created.
- Include the optional service-session-profile keyword to assign a profile to the service session. The service session profile includes additional attributes, such as the type of statistics to be captured for the service session.
- You can activate one subscriber session for a subscriber—and multiple service sessions for a particular subscriber session. If you create a second subscriber session for the same subscriber, only the newest subscriber session, with its services, is used.
- Example 1—Activate a service session for an existing subscriber
  `
  host1(config)#service-management owner-session aaa 573498 service-session “video(4500000, 192.168.10.3)”
  `
- Example 2—Activate multiple service sessions for an existing subscriber
  `
  host1(config)#service-management owner-session aaa 573498 service-session “video(4500000, 192.168.10.3)”
  host1(config)#service-management owner-session aaa 573498 service-session “tiered(1000000, 2000000)”
  host1(config)#service-management owner-session aaa 573498 service-session “voice(1000000, 10.10.10.1)”
  `
- Example 3—Include a service session profile when you activate a subscriber’s service session
  `
  host1(config)#service-management owner-session aaa 426777 service-session “video(4500000, 192.168.10.3)” service-session-profile vodISP1
  `
- Use the no version to deactivate service sessions based on owner information. See Using the CLI to Deactivate Subscriber Service Sessions for more information about deactivating subscriber service sessions.
- See service-management owner-session

service-management subscriber-session service-session

- Use to activate a service for a subscriber by creating a subscriber session and a service session.

  | Note: Always activate at least one service session for a subscriber session. The ability to create a subscriber session without a service session (by omitting the service-session keyword) is not currently supported.

- Use this command in Privileged Exec mode to create a dynamic subscriber session—dynamic sessions are deleted after a router reboot.
- Use this command in Global Configuration mode to create persistent subscriber sessions that are retained across reboots.
- Include the optional service-session-profile keyword to assign a profile to the service session. The service session profile includes additional attributes, such as the type of statistics to be captured for the service session.
- You can create one subscriber session for a subscriber—and multiple service sessions for a particular subscriber session. If you create a second subscriber session for the same subscriber, only the newest subscriber session, with its services, is used.
- Example 1—Activate a subscriber session with a single service session
  `
  host1(config)#service-management subscriber-session client1@isp1.com interface atm 4/0.1 service-session “video(4500000, 192.168.10.3)”
  `
- Example 2—Activate a single subscriber session with multiple service sessions
  `
  host1(config)#service-management subscriber-session client1@isp1.com interface atm 4/0.1 service-session “video(4500000, 192.168.10.3)”
  host1(config)#service-management subscriber-session client1@isp1.com interface atm 4/0.1 service-session “tiered(1000000, 2000000)”
  host1(config)#service-management subscriber-session client1@isp1.com interface atm 4/0.1 service-session “voice(1000000, 10.10.10.1)”
  `
- Example 3—Include a service session profile when you activate a subscriber’s service session
  `
  host1(config)#service-management subscriber-session client1@isp1.com interface atm 4/0.1 service-session “video(4500000, 192.168.10.3)” service-session-profile vodISP1
  `
- Use the no version to deactivate service sessions. See Using the CLI to Deactivate Subscriber Service Sessions for more information about deactivating subscriber service sessions.
- See service-management subscriber-session service-session

## Preprovisioning Services

Preprovisioning service sessions is a technique you can use to improve Service Manager’s performance. Typically, when you use a service definition to activate a subscriber’s service session, Service Manager uses resources to build that service. However, if you later use the same service definition to activate a service session for a second subscriber, Service Manager does not have to rebuild the service—it bases the new service on the service that it built for the first service session. After you deactivate the first session, Service Manager must build a new service for any subsequent subscribers.

Preprovisioning entails activating a service for a dummy user on the null interface. You can then use the preprovisioned service session to activate service sessions for actual subscribers. This technique improves performance because you only require Service Manager to build the service one time, then reuse the original service when you activate future subscriber service sessions.

To preprovision a service you use a command similar to the following example:

`

host1(config)#service-management subscriber-session dummy interface null service-session “tiered(1000000, 2000000)”

`

## Using Service Session Profiles

Service session profiles provide additional flexibility to the Service Manager application by enabling you to assign one or more supported attributes to a particular activation of a service.

For example, you might assign the same video service to two subscribers, but use different service session profiles to set different time limits for each subscriber’s service. One subscriber uses the video service for 5 hours (18000 seconds) while the other subscriber’s video service is for 10 hours (36000 seconds). Or, you might enable statistics on a subscriber’s voice service and disable statistics on the same subscriber’s video service.

You can create multiple service session profiles independent of the service activation process. Then, when you activate a service session, you specify the profile that you want to use with that particular service session—you can apply one profile to a service session.

You can configure the following attributes in service session profiles:

- statistics—Enables statistics and specifies the type of statistics you want to capture for the service. See Configuring Service Manager Statistics for additional information about capturing Service Manager statistics. You can specify the following types of statistics:
  - time—The service’s duration
  - volume-time—The service’s duration and traffic volume
- volume—Specifies that the service is automatically deactivated when the indicated traffic volume is exceeded.
- time—Specifies that the service is automatically deactivated when the indicated time period is exceeded.

  | Note: The volume and time attributes use values captured by the Service Manager statistics feature to determine when the threshold is exceeded. Service Manager collects time statistics by default—you must configure and enable volume statistics collection. See Configuring Service Manager Statistics .

To create or modify a service session profile:

1. Specify the name of the service session profile; doing this enters Service Session Profile Configuration mode.
   `
   host1(config)#service-management service-session-profile vodISP1
   host1(config-service-session-profile)#
   `
2. Specify the attributes you want to include in the profile.
   `
   host1(config-service-session-profile)#statistics volume-time
   host1(config-service-session-profile)#time 6000
   `
3. (Optional) To modify an existing profile, you can add new attributes or use the no version of a command to remove an attribute.
   `
   host1(config-service-session-profile)#no time
   `

service-management service-session-profile

- Use to create a new service session profile or to specify the name of an existing profile you want to modify, and to enter Service Session Profile Configuration mode.
- In Service Session Profile Configuration mode, you specify the attributes used in the service session profile, such as the maximum volume limit for the session and the maximum time the session can be used. You can also specify that Service Manager collect statistics for time, or volume, or both.
- Example
  `
  host1(config)#service-management service-session-profile vodISP1
  host1(config-service-session-profile)#
  `
- Use the no version to delete the service session profile.
- See service-management service-session-profile

statistics

- Use to enable statistics collection and to specify the type of statistics to collect.
  - Use the time keyword to collect statistics about the duration of the service session.
  - Use the volume-time keyword to collect statistics about both the volume of traffic and the duration of the service session.
- Example
  `
  host1(config)#service-management service-session-profile vodISP1
  host1(config-service-session-profile)#statistics volume-time
  `
- Use the no version to disable statistics collection.

  | Note: Service Manager statistics collection is a three-part procedure. You must configure statistics information in the service definition macro file, enable statistics collection by either RADIUS or the CLI, and also enable statistics collection for the policy referenced in the service macro using the statistics enabled keyword in the command used for policy attachment in the profile. See Configuring Service Manager Statistics .

- See statistics

time

- Use to specify the maximum amount of time that the service session can be active for the subscriber.
- The router immediately terminates the subscriber’s service session when the specified time is exceeded.
- The range is 0–16777251 seconds.
- Example
  `
  host1(config)#service-management service-session-profile vodISP1
  host1(config-service-session-profile)#time 6000
  `
- Use the no version to delete the time attribute from the service session profile.
- See time

volume

- Use to specify the maximum amount of bandwidth that can use the service.
- The router immediately terminates the subscriber’s service session when the specified traffic volume is exceeded.

  | Note: The volume attribute uses values captured by the Service Manager statistics feature to determine when the threshold is exceeded. Therefore, you must configure and enable statistics collection to use this attribute. See Configuring Service Manager Statistics .

- The range is 0–16777251MB.
- Example
  `
  host1(config)#service-management service-session-profile vodISP1
  host1(config-service-session-profile)#volume 1000000
  `
- Use the no version to delete the volume attribute from the service session profile.
- See volume

## Using the CLI to Deactivate Subscriber Service Sessions

The CLI supports several methods that enable you to manually deactivate service sessions. You can:

- Gracefully terminate all services or a specific service for a particular subscriber
- Gracefully terminate all service or a specific service associated with a particular owner
- Force the immediate termination of all of a subscriber’s sessions
- Use service session profiles to create time or volume thresholds for the service and deactivate the service when the threshold is reached. See Using Service Session Profiles.

  | Note: You can use the CLI commands described in this section to delete subscriber and service sessions that are created by either RADIUS or the CLI.

The Service Manager CLI commands enable you to use variations of the no service-management subscriber-session command to terminate service sessions.

### Gracefully Deactivating Subscriber Service Sessions

Use the following commands to gracefully deactivate subscriber’s services—you can deactivate a specific service for a subscriber, or you can delete a subscriber session, which deactivates all of the subscriber’s service sessions. We recommend you use this command to deactivate subscriber service sessions.

no service-management owner-session

- Use to gracefully deactivate service sessions for a subscriber based on owner information.
- Specify the owner name and owner ID of the service session you want to deactivate.
- Use the no version with the service-session keyword to deactivate the specified service session.
- Use the no version without the service-session keyword to delete the subscriber’s session and deactivate all of the subscriber’s service sessions.
- Example
  `
  host1(config)#no service-management owner-session aaa 426777 service-session “video(4500000, 192.168.10.3)”
  `
- This is the no version of the service-management owner-session command.
- See service-management owner-session

no service-management subscriber-session service-session

- Use to gracefully deactivate service sessions for a subscriber.
- Use the subscriber’s username and interface, not the subscriber session ID, for graceful deactivation.
- Use the no version without the service-session keyword to delete the subscriber’s session and deactivate all of the subscriber’s service sessions.
- Use the no version with the service-session keyword to deactivate the specified service session.
- Example
  `
  host1(config)#no service-management subscriber-session client1@isp1.com interface atm 4/0.1 service-session “tiered(1000000, 2000000)”
  `
- This is the no version of the service-management subscriber-session command.
- See service-management subscriber-session service-session

### Forcing Immediate Deactivation of Subscriber Service Sessions

Use the following command to force the immediate deactivation of the specified subscriber session—doing this deletes all active service sessions for the subscriber. We recommend this method if you encounter difficulty when you used the graceful deactivation method. Always use the graceful method first.

no service-management subscriber-session force

- Use to force the immediate termination of a subscriber session and to deactivate all services for the specified subscriber session.
- You must specify the subscriber session ID to use the force keyword to terminate the subscriber session.

  | Note: To determine the subscriber session ID of a session you want to deactivate, use the show service-management subscriber-session brief command. The display lists the IDs of all active subscriber sessions and the owner that created the session, such as AAA (RADIUS) or CLI.

- Example
  `
  host1(config)#no service-management subscriber-session 8 force
  `
- There is no affirmative version of this command; there is only a no version.
- See no service-management subscriber-session force

### Using Service Session Profiles to Deactivate Service Sessions

To terminate a subscriber service session when a threshold is reached, you create a service session profile that includes a time threshold, or a volume threshold, or both. Then, you attach the service session profile when you activate the service session. When the specified threshold is reached, the service session is terminated.

| Note: This feature is not supported by the service-management owner-session command. The service-management owner-session command only supports service session profiles when activating service sessions.

The following example shows the commands you might use to create a time threshold for deactivating a service session. See Using Service Session Profiles for information about using the time and volume keywords in service session profiles.

To create or modify a service session profile:

1. Specify the name of the service session profile and configure the threshold:
   `
   host1(config)#service-management service-session-profile vodISP1
   host1(config-service-session-profile)#time 6000
   host1(config-service-session-profile)#exit
   `
2. Include the service session profile when you activate the subscriber service session:
   `
   host1(config)#service-management subscriber-session client1@isp1.com interface atm 4/0.1 service-session “video(4500000, 192.168.10.3)” service-session-profile vodISP1
   `

[Contents] [Prev] [Next] [Index] [Report an Error]