[Contents] [Prev] [Next] [Index] [Report an Error]

# ip tcp ack-rst-and-syn

#### Syntax

[ no ] [ ip ] tcp ack-rst-and-syn [ vrf vrfName ]

#### Description

The ip keyword for tcp commands is now optional (with the exception of the ip tcp adjust-mss command, which is IPv4 specific). For information about this command and any other ip tcp command, see the tcp commands.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]