[Contents] [Prev] [Next] [Index] [Report an Error]

# l2tp drain destination

#### Syntax

[ no ] l2tp drain destination { destinationName
| [ virtual-router vrName ] ip ipAddress }

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Prevents the creation of new tunnels and sessions at a destination. This command works in conjunction with the l2tp shutdown destination command. Both commands affect the status of the administrative state of L2TP for the destination; the l2tp drain destination command sets the administrative state to drain. The no version allows the creation of new tunnels and sessions at a destination.

#### Options

- destinationName—Name the router assigns to the LNS
- vrName—Name of the virtual router on which the destination exists
- ipAddress—IP address of the LNS

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]