> - Download PDFs
> - tunnel-subscriber authentication
> - Related Topics
> - Configuring Tunnel Subscriber Authentication in the JUNOSe Broadband Access Configuration Guide

> # tunnel-subscriber authentication

> #### Syntax

> tunnel-subscriber authentication { enable | disable }

> no tunnel-subscriber authentication

> #### Release Information

> Command introduced in JUNOSe Release 9.1.0.

> #### Description

> Configures whether tunnel subscribers within the domain map are authenticated with the authentication server or are granted access without individual authentication. The no version restores the default condition, where users are not authenticated by an authentication server.

> #### Options

> - enable—Enables tunnel subscriber authentication by the authentication server
> - disable—Disables tunnel subscriber authentication by the authentication server; all users in the domain are granted access without individual authentication; this is the default condition

> #### Mode

> Domain Map Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.