[Contents] [Prev] [Next] [Index] [Report an Error]

# disable-switch-on-error

#### Syntax

[ no ] disable-switch-on-error

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Prevents the redundant SRP module from taking over if the primary SRP module experiences a software failure or if you push the reset button on the primary SRP module. Issue the sync command immediately before you issue this command. The no version restores the default situation, in which the redundant SRP module takes over if the primary SRP module experiences a failure.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]