[Contents] [Prev] [Next] [Index] [Report an Error]

## snmpPduAudit

#### Description

SNMP PDUs

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

None

#### Notice Log

None

#### Info

Identifies the following fields in all SNMP PDUs sent to the E-series router and all trap PDUs that leave the system: source and destination IP address, PDU type, snmpVersion, requested, errorStatus, errorIndex, variable count, variable object identifier and data

#### Debug

None

#### Filter

None

[Contents] [Prev] [Next] [Index] [Report an Error]