[Contents] [Prev] [Next] [Index] [Report an Error]

# ip dhcp-server

#### Syntax

ip dhcp-server dhcpServerAddress [ adminStatus ]

no ip dhcp-server [ dhcpServerAddress [ adminStatus ] ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Adds the IP address of a single DHCP server to the list of DHCP servers from which the router can request addresses to allocate to remote users. A maximum of five DHCP servers can be specified. The no version removes the specified DHCP server or removes all DHCP servers from the list.

#### Options

- dhcpServerAddress—IP address of the DHCP server that will allocate addresses for remote users
- adminStatus—One of the following options:
  - disable—Disables the DHCP server
  - drain—Drains the DHCP server

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]