[Contents] [Prev] [Next] [Index] [Report an Error]

# show tcp resequence-buffers

#### Syntax

show [ ip ] tcp resequence-buffers [ vrf vrfName ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0
ip keyword made optional in JUNOSe Release 7.2.0.

#### Description

Displays the configuration, current per-VR and per-router state of the TCP resequencing buffer management functions.

#### Options

- vrfName—Name of the VRF

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]