[Contents] [Prev] [Next] [Index] [Report an Error]

# l2tp tunnel short-drain-timeout

#### Syntax

l2tp tunnel short-drain-timeout [ timeOutValue ]

no l2tp tunnel short-drain-timeout

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Configures the amount of time a disconnected LAC L2TP tunnel waits (the drain timeout) before restarting after a restart request is received. The no version restores the default setting.

#### Options

- timeOutValue—Short drain timeout in seconds, in the range 0–31; default value is 2 seconds

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]