[Contents] [Prev] [Next] [Index] [Report an Error]

# Creating Policy Lists for IPv6

The following example creates an IPv6 policy list named routeForIPv6. For information about creating the CLACL used in this example, see the previous sections.

1. Create the policy list routeForIPv6.
   `
   host1(config)#ipv6 policy-list routeForIPv6
   host1(config-policy-list)#
   `
2. Create the classification group for the CLACL named ipv6tc67 and assign the precedence to the classification group.
   `
   host1(config-policy-list)#classifier-group ipv6tc67 precedence 75
   host1(config-policy-list-classifier-group)#
   `
3. Add a rule to color packets as red, and a second rule that sets the traffic class field of the packets to 7.
   `
   host1(config-policy-list-classifier-group)#color red
   host1(config-policy-list-classifier-group)#mark tcfield 7
   `
4. Exit Policy List Configuration mode to save the configuration.
   `
   host1(config-policy-list-classifier-group)#exit
   host1(config-policy-list)#exit
   host1(config)#
   `
5. Display the policy list.

       host1#show policy-list routeForIPv6

                                         Policy Table
                                         ------ -----
       IPv6 Policy routeForIPv6
          Administrative state: enable
          Reference count:      0
          Classifier control list: ipv6tc67, precedence 75
             color red
             mark tc-precedence 7

You use the exception http-redirect command to create an exception rule within a policy classifier group to specify the client application for the destination of packets rather than forwarding them using the forwarding controller (FC).

In lower-numbered releases, the exception http-redirect command only supported the creation of exception rules within IPv4 policy lists. You can now configure the exception http-redirect command to create exception rules within IPv4 and IPv6 policy lists.

The following example creates an IPv6 policy list, epIPv6 for the http-redirect exception:

1. Create the policy list epIPv6.
   `
   host1(config)#ipv6 policy-list epIPv6
   host1(config-policy-list)#
   `
2. Create the classification group to match all packets.
   `
   host1(config-policy-list)#classifier-group *
   host1(config-policy-list-classifier-group)#
   `
3. Create an exception policy for http-redirect.
   `
   host1(config-policy-list-classifier-group)#exception http-redirect
   `
4. Exit Policy List Configuration mode to save the configuration.
   `
   host1(config-policy-list-classifier-group)#exit
   host1(config-policy-list)#exit
   host1(config)#
   `
5. Display the policy list.

       host1#show policy-list epIPv6

                                         Policy Table
                                         ------ -----
       IPv6 Policy epIPv6
          Administrative state: enable
          Reference count:      0
          Classifier control list: *, precedence 100
             exception http-redirect

#### Related Topics

- ipv6 policy-list
- exception http-redirect

[Contents] [Prev] [Next] [Index] [Report an Error]