[Contents] [Prev] [Next] [Index] [Report an Error]

# rtr schedule

#### Syntax

[ no ] rtr schedule rtrIndex

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the RTR time parameters for an RTR operation. The no version stops the operation by putting it in the pending state. The no version also resets the restart-time attribute and the life attribute.

#### Options

- rtrIndex—Number of the operation to be configured, in the range 1–4294967295; no default

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]