[Contents] [Prev] [Next] [Index] [Report an Error]

# ip igmp querier

#### Syntax

[ no ] ip igmp querier

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies that the interface will act as a querier when you configure IGMPv1 on an interface; this is the default behavior. The no version specifies that this interface will not issue query packets.

| Note: This command is valid only for interfaces on configured with IGMPv1.

#### Mode

Interface Configuration, Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]