[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Rate Statistics

To gather rate statistics:

1. Create the statistics profile.
   `
   host1(config)#statistics-profile statpro-5
   `
2. Set the length of time during which statistics are counted.
   `
   host1(config-statistics-profile)#rate-period 45
   Rate period range is 1–43200 seconds.
   `
3. Reference the statistics profile by a QoS profile.
   `
   host1(config)#qos-profile qospro-3
   host1(config-qos-profile)#ip queue traffic-class tc1 scheduler-profile sp1 statistics-profile statpro-5
   `
4. Attach the QoS profile to the appropriate interface.
   `
   host1(config)#interface gigabitEthernet 1/0
   host1(config-subif)#qos-profile qospro-3
   host1(config-subif)#exit
   `
5. (Optional) Display the rate statistics.
   `
   host1#show egress-queue rates interface gigabitEthernet 1/0
   `

#### Related Topics

- Configuring Statistic Profiles for QoS
- Configuring a QoS Profile
- Monitoring QoS Statistics for Rates and Events
- interface command
- qos-profile command
- queue command
- rate-period command
- statistics-profile command

[Contents] [Prev] [Next] [Index] [Report an Error]