[Contents] [Prev] [Next] [Index] [Report an Error]

# rtr reaction-configuration operation-failure

#### Syntax

rtr reaction-configuration rtrIndex operation-failure [ operationFailureValue ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables operation-failure reaction. When the type of RTR entry is echo, you can also configure a value that triggers the operation-failure trap. When the type of RTR entry is pathEcho, you cannot configure the operation-failure trap. There is no no version. See the no rtr reaction-configuration command.

#### Options

- rtrIndex—Number of the operation to be configured, in the range 1–4294967295
- operationFailureValue—Number, in the range 0–15; default value is 1

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]