> - Download PDFs
> - tacacs-server host

> # tacacs-server host

> #### Syntax

> tacacs-server host ipAddress [ port portNumber ]
> [ timeout timeoutValue ] [ key keyValueString ] [ primary ]

> no tacacs-server host ipAddress

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Adds or deletes a host to or from the list of TACACS+ servers. If the host is not assigned as the primary host, the router assigns an existing host as the primary. The no version deletes the host from the list of TACACS+ servers.

> #### Options

> - ipAddress—IP address of the TACACS+ server
> - portNumber—TACACS+ server’s TCP port number in the range 1–655535
> - timeoutValue—Response timeout interval for the TACACS+ client to server exchange; number in the range 1–255; default value is 5
> - keyValueString—Secret used in TACACS+ client to server exchange; string of up to 100 characters
> - primary—Assigns the host as the primary host

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.