[Contents] [Prev] [Next] [Index] [Report an Error]

# aaa virtual-router

#### Syntax

aaa virtual-router indexInteger vrName

no aaa virtual-router indexInteger

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

For AAA broadcast accounting, adds a virtual router to a virtual router group. The no version with the indexInteger parameter removes a specific virtual router from the virtual router group.

#### Options

- indexInteger—Number in the range 1–4 that indicates the virtual router's listing in the virtual router group; the indexInteger is used in the no version of the command to delete a particular virtual router from the group
- vrName—Name of virtual router that can receive AAA broadcast accounting packets.

#### Mode

VR Group Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]